

Installation Instruction:

This CD-Rom contains
	USB hardware driver
	DataLogger download program
	User manual for PT250+


1. Please install first the USB-driver from the "Driver" directory. 
   Click on CP210x_VCP_Win_XP_S2K3_Vista_7.exe

2. Install the download program from the directory "DataLogger". 
   Click on Seaward_Solar_DatalLogger_Installer_1_0_2.exe


The USB-hardware driver is installed automatically on a free COM-Port as soon as 
  the PT250+ device is connected via USB-interface to the PC.

Then run the DataLogger program to transfer data from the device to your PC.

There is more information on how to transfer data from your tester under the Help menu in DataLogger.

The User Manual for the PT250+ is in directory "Manuals".


Further information and support under: 		www.Seaward.co.uk/faqs




